	Checklist Approach for “Turn-it-off” Measures

	Measure
	Observation
	Recommendation

	Reduce HVAC schedules
	
	

	Holiday scheduling
	
	

	Optimal start/stop
	
	

	Chiller outdoor air enabled
	
	

	Heating system outdoor air enabled
	
	

	Keep air handlers (AHU) off during night heating cycles 
	
	

	Reduce lighting schedules
	
	

	Exterior lighting – schedule off late at night
	
	

	De-lamping
	
	

	Snowmelt system control
	
	

	Pump shutdown when there is no load
	
	

	Checklist Approach for “Turn-it-down” Measures

	Measure
	Observation
	Recommendation

	Static pressure reset
	
	

	Night setback
	
	

	Chilled water differential pressure reset
	
	

	Hot water differential pressure reset
	
	

	Chilled water temperature reset
	
	

	Hot water temperature reset
	
	

	Condenser water temperature reset
	
	

	Chiller staging
	
	

	AHU freeze protection
	
	

	Checklist Approach for “Mitigate Simultaneous Heating and Cooling” Measures

	Measure
	Observation
	Recommendation

	Supply air temperature reset
	
	

	Reduce variable air volume (VAV) box minimum airflow setpoints
	
	

	Enable/fix economizers
	
	

	Thermostat setpoints and deadbands
	
	

	Dedicated outdoor air system (DOAS): supply air temperature reset
	
	

	DOAS: heat recovery control
	
	

	Eliminate fighting thermostats
	
	

	Night purge
	
	

	Checklist Approach for “Reduce Outdoor Air and Infiltration” Measures

	Measure
	Observation
	Recommendation

	Demand control ventilation (DCV)
	
	

	Reduced minimum outdoor air
	
	

	Building pressurization control
	
	

	Close OA dampers at night/weekends/morning start-up
	
	

	Exhaust fan control and scheduling
	
	

	Garage supply/exhaust fan control
	
	



