<html><head></head><body><pre style="word-wrap: break-word; white-space: pre-wrap;">################################################################################
# DHSVM INPUT FILE FORMAT
################################################################################
# The file is organized in sections [...], which contain key = entry pairs.  
# The file is free format, in that correct reading of the file is not dependent 
# on spaces and/or the order of the key-entry pairs within a section.  
# The keys are not case-sensitive, but the entries are, because filenames on a 
# UNIX platform are case-sensitive.  
# Comments are preceded by a '#', and run from the occurrence of '#' till the 
# end of the line. You can comment out an entire line (like in this 
# header), or you can place a comment after an entry.  
# It is important to place the key-entry pair in the correct section, since it 
# will not be found if it is in another section.  
# The easiest way to make the input file is to fill out this default template.  
# Since DHSVM will only use the keys that it requires you do not have to worry 
# about empty entries for keys that are not needed. For example, if you are 
# running the model in point mode, you do not have to fill out the routing 
# section.  If you have already filled it out you can leave it, since DHSVM will 
# not use the information.  This allows easy switching between point and basin 
# mode.  
# For more information about the specific entries see the DHSVM web page

################################################################################
# OPTIONS SECTION 
################################################################################
[OPTIONS]                                 # Model Options
Format               = BIN                # BIN, BYTESWAP or NETCDF
Extent               = BASIN              # POINT or BASIN
Gradient             = WATERTABLE 	  # TOPOGRAPHY or WATERTABLE
Flow Routing         = NETWORK            # UNIT_HYDROGRAPH or NETWORK
Sensible Heat Flux   = FALSE              # TRUE or FALSE
Sediment             = FALSE		  # TRUE or FALSE
Sediment Input File  =			  # path for sediment configuration file
Overland Routing     = CONVENTIONAL	  # CONVENTIONAL or KINEMATIC
Infiltration	     = STATIC		  # Static or Dynamic
Interpolation        = VARCRESS           # NEAREST or INVDIST or VARCRESS
MM5                  = FALSE		  # TRUE or FALSE
QPF                  = FALSE              # TRUE or FALSE
PRISM                = FALSE              # TRUE or FALSE
PRISM data path      =                    # path for PRISM files
PRISM data extension = bin                # file extension for PRISM files
Canopy radiation attenuation mode = FIXED # FIXED or VARIABLE
Shading              = TRUE    	          # TRUE or FALSE
Shading data path    = /nfs/electric/raid/ning/Test_SpringBrook/input/Shadow
Shading data extension = hourly.bin       # file extension for shading files 
Skyview data path    = /nfs/electric/raid/ning/Test_SpringBrook/input/SkyView.bin
Snotel               = FALSE              # TRUE or FALSE
Outside              = TRUE	          # TRUE or FALSE
Rhoverride           = FALSE              # TRUE or FALSE
Precipitation Source = STATION            # STATION or RADAR
Wind Source          = STATION            # STATION or MODEL
Temperature lapse rate   = CONSTANT       # CONSTANT or VARIABLE
Precipitation lapse rate = CONSTANT       # CONSTANT, MAP, or VARIABLE
Cressman radius      = 10                 # in model pixels
Cressman stations    =  4                 # number of stations

################################################################################
# MODEL AREA SECTION
################################################################################
[AREA]                                    # Model area
Coordinate System    = UTM                # UTM or USER_DEFINED
Extreme North        = 5253547.579        # Coordinate for northern edge of grid
Extreme West         = 557427.379         # Coordinate for western edge of grid
Center Latitude      = 47.408             # Central parallel of basin 
Center Longitude     = -122.204           # Central meridian of basin 
Time Zone Meridian   = -120.0             # Time zone meridian for area 
Number of Rows       = 213                # Number of rows
Number of Columns    = 164                # Number of columns
Grid spacing         = 30                 # Grid resolution in m 
Point North          =                    # North coordinate for point model if Extent = POINT 
Point East           =                    # East coordinate for point modelif Extent = POINT 

################################################################################
# TIME SECTION
################################################################################
[TIME]                                    # Model period
Time Step            = 1                  # Model time step (hours)
Model Start          = 10/01/1995-00      # Model start time (MM/DD/YYYY-HH)
Model End            = 10/15/1995-00      # Model end time (MM/DD/YYYY-HH)

################################################################################
# CONSTANTS SECTION
################################################################################
[CONSTANTS]                               # Model constants
Ground Roughness     = 0.02               # Roughness of soil surface (m)
Snow Roughness       = 0.01               # Roughness of snow surface (m)
Rain Threshold       = -1.0               # Minimum temperature at which rain 
					  # occurs (C)
Snow Threshold       = 0.5                # Maximum temperature at which snow 
					  # occurs (C)
Snow Water Capacity  = 0.03               # Snow liquid water holding capacity 
					  # (fraction)
Reference Height     = 45.0               # Reference height (m)
Rain LAI Multiplier  = 0.0001             # LAI Multiplier for rain interception
Snow LAI Multiplier  = 0.0005             # LAI Mulitplier for snow interception
Min Intercepted Snow = 0.005              # Intercepted snow that can only be 
					  # melted (m)
Outside Basin Value  = 0                  # Value in mask that indicates outside 
					  # the basin
Temperature Lapse Rate   = -0.0065        # Temperature lapse rate (C/m)
Precipitation Lapse Rate =  0.0000   	  # Precipitation lapse rate (m/m)
################################################################################
# TERRAIN INFORMATION SECTION
################################################################################
[TERRAIN]                                 # Terrain information
DEM File             = /nfs/electric/raid/ning/Test_SpringBrook/input/springbrook.dem.bin
Basin Mask File      = /nfs/electric/raid/ning/Test_SpringBrook/input/springbrook.mask.bin 

################################################################################
# ROUTING SECTION
################################################################################
[ROUTING]                                 # Routing information. This section is 
                                          # only relevant if the Extent = BASIN

################ STREAM NETWORK ################################################
# The following three fields are only used if Flow Routing = NETWORK

Stream Map File      =  /nfs/electric/raid/ning/Test_SpringBrook/input/springbrook.stream.map
Stream Network File  =  /nfs/electric/raid/ning/Test_SpringBrook/input/springbrook.stream.network 
Stream Class File    =  /nfs/electric/raid/ning/Test_SpringBrook/input/adjust.classfile 

################ ROAD NETWORK ##################################################
# The following three fields are only used if Flow Routing = NETWORK and there
# is a road network

#Road Map File        =                    # path for road map file
#Road Network File    =                    # path for road network file
#Road Class File      =                    # path for road network file

################ UNIT HYDROGRAPH ###############################################
# The following two fields are only used if Flow Routing = UNIT_HYDROGRAPH

Travel Time File     =                    # path for travel time file
Unit Hydrograph File =                    # path for unit hydrograph file

###############################################################################
# METEOROLOGY SECTION 
################################################################################
[METEOROLOGY]                             # Meteorological stations
Number of Stations = 1                   # Number of meteorological stations

Station Name 1 = seatac_-122.21875_47.40625_combo 
#Seatac airport location
North Coordinate 1 = 5236598.4 
East Coordinate 1 = 561258.1
Elevation 1 = 121.90 
Station File 1 = /nfs/electric/raid/ning/MET/vic_met/urban_met_stations/urban12113346_12113349/hrly.met02_95_03_seatac.prcp_windprofile_70m
################ MM5 ###########################################################
# The following block only needs to be filled out if MM5 = TRUE.  In that case
# This is the ONLY block that needs to be filled out

MM5 Start              =                  # Start of MM5 file (MM/DD/YYYY-HH),
MM5 Rows               =
MM5 Cols               =
MM5 Extreme North      =
MM5 Extreme West       = 
MM5 DY                 =

# MM5 met files
MM5 Temperature File   = 
MM5 Humidity File      = 
MM5 Wind Speed File    = 
MM5 Shortwave File     = 
MM5 Longwave File      = 
MM5 Pressure File      = 
MM5 Precipitation File = 
MM5 Terrain File       =
MM5 Temp Lapse File    =

# For each soil layer make a key-entry pair as below (n = 1, ..,
# Number of Soil Layers)

MM5 Soil Temperature File 0 = 
MM5 Soil Temperature File 1 = 
MM5 Soil Temperature File 2 = 

############### RADAR ##########################################################
# The following block only needs to be filled out if Precipitation Source = 
# RADAR.  
Radar Start            =
Radar File             =
Radar Extreme North    =
Radar Extreme West     =
Radar Number of Rows   =
Radar Number of Columns = 
Radar Grid Spacing     =

################ Wind ##########################################################
# The following block only needs to be filled out if Wind Source = MODEL
Number of Wind Maps    =
Wind File Basename     =
Wind Map Met Stations  =

################ Precipitation lapse rate ######################################
# The following block only needs to be filled out if Precipitation lapse rate 
# = MAP
Precipitation lapse rate =

################################################################################
# SOILS INFORMATION SECTION
################################################################################
[SOILS]                                   # Soil information
Soil Map File	     = /nfs/electric/raid/ning/Test_SpringBrook/input/springbrook.soilclass.bin
Soil Depth File      = /nfs/electric/raid/ning/Test_SpringBrook/input/springbrook.soildepth.bin

Number of Soil Types = 3                

################################## SOIL 1 #########################################################
Soil Description       1 = SAND
Lateral Conductivity   1 = 0.1               
Exponential Decrease   1 = 3.0       
Maximum Infiltration   1 = 2.0e-1     
Capillary Drive        1 = 0.09         # http://www.tucson.ars.ag.gov/icrw/Proceedings/Hantush.pdf
					# the value must be filled out but is not used in computation
					# if INFILTRATION = STATIC
Surface Albedo         1 = 0.1       
Number of Soil Layers  1 = 3       
Porosity               1 =  .43 .43 .43
Pore Size Distribution 1 =  .24 .24 .24
Bubbling Pressure      1 =  .07 .07 .07 
Field Capacity         1 =  .08 .08 .08 
Wilting Point          1 =  .03 .03 .03 
Bulk Density           1 = 1492. 1492. 1492. 
Vertical Conductivity  1 = 5.0E-1 5.0E-1 5.0E-1
Thermal Conductivity   1 = 7.114  6.923 6.923
Thermal Capacity       1 = 1.4e6  1.4e6 1.4e6
Mannings n             1 = 0.013         # the value must be filled out but is not used in computation
				         # if routing = conventional
################################## SOIL 2 #########################################################
Soil Description       2 = LOAMY SAND    
Lateral Conductivity   2 = 0.03              
Exponential Decrease   2 = 3.5      
Maximum Infiltration   2 = 3.0e-2      
Capillary Drive        2 = 0.12
Surface Albedo         2 = 0.1       
Number of Soil Layers  2 = 3       
Porosity               2 =  .42 .42 .42
Pore Size Distribution 2 =  .25 .25 .25
Bubbling Pressure      2 =  .09 .09 .09
Field Capacity         2 =  .10 .10 .10
Wilting Point          2 =  .06 .06 .06
Bulk Density           2 = 1520. 1520. 1520.
Vertical Conductivity  2 = 3.0E-2 3.0E-2 3.0E-2
Thermal Conductivity   2 = 7.114  6.923 7.0
Thermal Capacity       2 = 1.4e6  1.4e6 1.4e6
Mannings n             2 = 0.013 
################################## SOIL 3 #########################################################
Soil Description       3 = SANDY LOAM      
Lateral Conductivity   3 = 0.01     
Exponential Decrease   3 = 3.0       
Maximum Infiltration   3 = 3e-5    
Capillary Drive        3 = 0.09  
Surface Albedo         3 = 0.1       
Number of Soil Layers  3 = 3       
Porosity               3 =  .40 .40 .40
Pore Size Distribution 3 =  .21 .21 .21
Bubbling Pressure      3 =  .15 .15 .15
Field Capacity         3 =  .21 .21 .21
Wilting Point          3 =  .09 .09 .09
Bulk Density           3 = 1569. 1569. 1569.
Vertical Conductivity  3 = 0.01 0.01 0.01
Thermal Conductivity   3 = 7.114  6.923 7.0 
Thermal Capacity       3 = 1.4e6  1.4e6 1.4e6
Mannings n             3 = 0.013
################################################################################
# VEGETATION INFORMATION SECTION
################################################################################
[VEGETATION]

Vegetation Map File        = /nfs/electric/raid/ning/Test_SpringBrook/input/springbrook.lc.bin

Number of Vegetation Types = 14           # Number of different vegetation types

################ VEGETATION 1 ##################################################
Vegetation Description   1 = Dense Urban (&gt;75%) 
Impervious Fraction      1 = 0.75
Detention Fraction       1 = 0.2
Detention Decay          1 = 0.3
IMPERVIOUS SURFACE ROUTING FILE = /nfs/electric/raid/ning/Test_SpringBrook/input/surface.routing.txt
Overstory Present        1 = FALSE  
Understory Present       1 = TRUE    
Fractional Coverage      1 = 	   
Hemi Fract Coverage      1 = 
Trunk Space              1 =        
Clumping Factor          1 =
Leaf Angle A             1 =
Leaf Angle B             1 =
Scattering Parameter     1 =
Aerodynamic Attenuation  1 =        
Radiation Attenuation    1 =        
Max Snow Int Capacity    1 =  
Snow Interception Eff    1 = 
Mass Release Drip Ratio  1 = 
Height                   1 = 0.2
Overstory Monthly LAI    1 = 
Understory Monthly LAI   1 = 0.5 0.5 0.5 0.5 0.5 1.5 1.5 1.5 1.5 0.5 0.5 0.5 
Maximum Resistance       1 = 3000.  
Minimum Resistance       1 = 340.   
Moisture Threshold       1 = 0.33 
Vapor Pressure Deficit   1 = 4000 
Rpc                      1 = .108
Overstory Monthly Alb    1 = 
Understory Monthly Alb   1 = 0.4 0.4 0.4 0.4 0.4 0.4 0.4 0.4 0.4 0.4 0.4 0.4
Number of Root Zones     1 = 3		
Root Zone Depths         1 = 0.10 0.25 0.40 
Overstory Root Fraction  1 = 0.20 0.40 0.40
Understory Root Fraction 1 = 0.40 0.60 0.00  

Vegetation Description   2 = Light/medium Urban (&lt;75%) 
Impervious Fraction      2 = 0.25
Detention Fraction       2 = 0.4
Detention Decay          2 = 0.2
IMPERVIOUS SURFACE ROUTING FILE = /net/flouric/usr1/lancuo/dhsvm/puget_sound_dhsvm/urban_basins/urban12113346/input/surface.routing.txt
Overstory Present        2 = FALSE
Understory Present       2 = TRUE   
Fractional Coverage      2 =  
Hemi Fract Coverage      2 = 
Clumping Factor          2 =			
Leaf Angle A             2 =
Leaf Angle B             2 =			
Scattering Parameter     2 =
Trunk Space              2 =  
Clumping Factor          2 =			
Leaf Angle A             2 =
Leaf Angle B             2 =			
Scattering Parameter     2 =
Trunk Space              2 =  
Aerodynamic Attenuation  2 = 
Radiation Attenuation    2 = 
Max Snow Int Capacity    2 = 
Snow Interception Eff    2 = 
Mass Release Drip Ratio  2 = 
Height                   2 = 0.2
Overstory Monthly LAI    2 = 
Understory Monthly LAI   2 = 1.0 1.0 1.0 1.0 1.0 3.0 3.0 3.0 3.0 1.0 1.0 1.0
Maximum Resistance       2 = 3000.
Minimum Resistance       2 = 300
Moisture Threshold       2 = 0.33     
Vapor Pressure Deficit   2 = 4000    
Rpc                      2 = 0.108
Overstory Monthly Alb    2 = 
Understory Monthly Alb   2 = 0.20 0.20 0.20 0.20 0.20 0.20 0.20 0.20 0.20 0.20 0.20 0.20
Number of Root Zones     2 = 3		   
Root Zone Depths         2 = 0.10 0.25 0.40   
Overstory Root Fraction  2 = 0.20 0.40 0.40
Understory Root Fraction 2 = 0.40 0.60 0.00    
   
Vegetation Description   3 = Bareground 
Impervious Fraction      3 = 0.0
Detention Fraction       3 = 0
Detention Decay          3 = 0
Overstory Present        3 = FALSE 
Understory Present       3 = FALSE   
Fractional Coverage      3 = 	   
Hemi Fract Coverage      3 = 
Clumping Factor          3 =			
Leaf Angle A             3 =
Leaf Angle B             3 =			
Scattering Parameter     3 =
Trunk Space              3 =  
Aerodynamic Attenuation  3 = 
Radiation Attenuation    3 =  
Max Snow Int Capacity    3 =  
Snow Interception Eff    3 = 
Mass Release Drip Ratio  3 = 
Height                   3 = 
Overstory Monthly LAI    3 = 
Understory Monthly LAI   3 = 
Maximum Resistance       3 =  
Minimum Resistance       3 = 
Moisture Threshold       3 = 
Vapor Pressure Deficit   3 =  
Rpc                      3 = 
Overstory Monthly Alb    3 = 
Understory Monthly Alb   3 = 
Number of Root Zones     3 = 3		
Root Zone Depths         3 = 0.10 0.25 0.40 
Overstory Root Fraction  3 = 0.20 0.40 0.40            
Understory Root Fraction 3 = 0.40 0.60 0.00  

Vegetation Description   4 = Dry Ground
Impervious Fraction      4 = 0.0
Detention Fraction       4 = 0
Detention Decay          4 = 0
Overstory Present        4 = FALSE    
Understory Present       4 = TRUE  
Fractional Coverage      4 =     
Hemi Fract Coverage      4 = 
Clumping Factor          4 =
Leaf Angle A             4 =
Leaf Angle B             4 =
Scattering Parameter     4 =
Trunk Space              4 =  0.38  
Aerodynamic Attenuation  4 = 
Radiation Attenuation    4 = 
Max Snow Int Capacity    4 = 
Snow Interception Eff    4 = 
Mass Release Drip Ratio  4 = 
Height                   4 = 0.5
Overstory Monthly LAI    4 = 
Understory Monthly LAI   4 = 0.5 0.5 0.5 0.5 0.5 6.0 6.0 6.0 6.0 0.5 0.5 0.5 
Maximum Resistance       4 = 600.
Minimum Resistance       4 = 320 
Moisture Threshold       4 = 0.33 
Vapor Pressure Deficit   4 = 4000 
Rpc                      4 = 0.108
Overstory Monthly Alb    4 = 
Understory Monthly Alb   4 = 0.19 0.19 0.9 0.19 0.19 0.19 0.19 0.19 0.19 0.19 0.19 0.19
Number of Root Zones     4 = 3		   
Root Zone Depths         4 = 0.10 0.25 0.40   
Overstory Root Fraction  4 = 0.20 0.40 0.40    
Understory Root Fraction 4 = 0.40 0.60 0.00    

Vegetation Description   5 = Native Grass
Impervious Fraction      5 = 0.0
Detention Fraction       5 = 0
Detention Decay          5 = 0
Overstory Present        5 = TRUE
Understory Present       5 = TRUE             
Fractional Coverage      5 = 0.5
Hemi Fract Coverage      5 = 0.5 
Clumping Factor          5 =
Leaf Angle A             5 =
Leaf Angle B             5 =
Scattering Parameter     5 =
Trunk Space              5 = 0.4
Aerodynamic Attenuation  5 = 0.3
Radiation Attenuation    5 = 0.1
Max Snow Int Capacity    5 = 0.003		  
Snow Interception Eff    5 = 0.6
Mass Release Drip Ratio  5 = 0.4
Height                   5 = 20.0 0.5      
Overstory Monthly LAI    5 = 2.0 2.0 2.0 2.0 2.0 6.0 6.0 6.0 6.0 2.0 2.0 2.0
Understory Monthly LAI   5 = 1.0 1.0 1.0 1.0 1.0 3.3 3.3 3.3 3.3 1.0 1.0 1.0
Maximum Resistance       5 = 1000 600.  
Minimum Resistance       5 = 280 200.    
Moisture Threshold       5 = 0.33 0.33     
Vapor Pressure Deficit   5 = 4000  4000    
Rpc                      5 = 0.108 0.108
Overstory Monthly Alb    5 = 0.15 0.15 0.15 0.15 0.15 0.14 0.14 0.14 0.14 0.15 0.15 0.15 
Understory Monthly Alb   5 = 0.18 0.18 0.18 0.18 0.18 0.18 0.18 0.18 0.18 0.18 0.18 0.18 
Number of Root Zones     5 = 3 		   
Root Zone Depths         5 = 0.10 0.25 0.40   
Overstory Root Fraction  5 = 0.20 0.40 0.40      
Understory Root Fraction 5 = 0.40 0.60 0.00    

Vegetation Description   6 = Grass/crop/shrub
Impervious Fraction      6 = 0.0
Detention Fraction       6 = 0
Detention Decay          6 = 0
Overstory Present        6 = FALSE 
Understory Present       6 = TRUE             
Fractional Coverage      6 =  
Hemi Fract Coverage      6 = 
Clumping Factor          6 =
Leaf Angle A             6 =
Leaf Angle B             6 =
Scattering Parameter     6 =
Trunk Space              6 = 
Aerodynamic Attenuation  6 = 
Radiation Attenuation    6 =  
Max Snow Int Capacity    6 = 		  
Snow Interception Eff    6 =  
Mass Release Drip Ratio  6 = 
Height                   6 = 1.0
Overstory Monthly LAI    6 = 
Understory Monthly LAI   6 = 1.0 1.0 1.0 1.0 1.0 5.25 5.25 5.25 5.25 5.25 1.0 1.0
Maximum Resistance       6 = 600.  
Minimum Resistance       6 = 280    
Moisture Threshold       6 = 0.33     
Vapor Pressure Deficit   6 = 4000     
Rpc                      6 = .108
Overstory Monthly Alb    6 = 
Understory Monthly Alb   6 = 0.24 0.24 0.23 0.22 0.21 0.20 0.20 0.20 0.22 0.23 0.24 0.24
Number of Root Zones     6 = 3 		   
Root Zone Depths         6 = 0.10 0.25 0.40   
Overstory Root Fraction  6 = 0.20 0.40 0.40      
Understory Root Fraction 6 = 0.40 0.60 0.00    

Vegetation Description   7 = Mixed/deciduous Forest
Impervious Fraction      7 = 0.0
Detention Fraction       7 = 0
Detention Decay          7 = 0
Overstory Present        7 = TRUE       
Understory Present       7 = TRUE             
Fractional Coverage      7 = 0.85         
Hemi Fract Coverage      7 = 0.85
Clumping Factor          7 =
Leaf Angle A             7 =
Leaf Angle B             7 =
Scattering Parameter     7 =
Trunk Space              7 = 0.45           
Aerodynamic Attenuation  7 = 2.0          
Radiation Attenuation    7 = 0.1875         
Max Snow Int Capacity    7 = 0.01225		  
Snow Interception Eff    7 = 0.6              
Mass Release Drip Ratio  7 = 0.4             
Height                   7 = 25.0 0.5      
Overstory Monthly LAI    7 = 3.0 3.0 3.0 3.0 3.0 8.5 8.5 8.5 8.5 3.0 3.0 3.0
Understory Monthly LAI   7 = 2.0 2.0 2.0 2.0 2.0 8.5 8.5 8.5 8.5 2.0 2.0 2.0
Maximum Resistance       7 = 1500. 1000.  
Minimum Resistance       7 = 666.6 823.4
Moisture Threshold       7 = 0.33 0.13     
Vapor Pressure Deficit   7 = 4000 4000     
Rpc                      7 = .108 .108
Overstory Monthly Alb    7 = 0.27 0.27 0.25 0.25 0.22 0.21 0.21 0.21 0.21 0.22 0.24 0.26
Understory Monthly Alb   7 = 0.175 0.175 0.175 0.175 0.175 0.175 0.175 0.175 0.175 0.175 0.175 0.175
Number of Root Zones     7 = 3 		   
Root Zone Depths         7 = 0.10 0.25 0.40   
Overstory Root Fraction  7 = 0.20 0.40 0.40      
Understory Root Fraction 7 = 0.40 0.60 0.00      

Vegetation Description   8 = Conifer Forest 
Impervious Fraction      8 = 0.0
Detention Fraction       8 = 0
Detention Decay          8 = 0
Overstory Present        8 = TRUE        
Understory Present       8 = TRUE             
Fractional Coverage      8 = 0.9         
Hemi Fract Coverage      8 = 0.9
Clumping Factor          8 =
Leaf Angle A             8 =
Leaf Angle B             8 =
Scattering Parameter     8 =
Trunk Space              8 = 0.5         
Aerodynamic Attenuation  8 = 2.5     
Radiation Attenuation    8 = 0.16         
Max Snow Int Capacity    8 = 0.03 
Snow Interception Eff    8 = 0.6              
Mass Release Drip Ratio  8 = 0.4             
Height                   8 = 43.3 0.5
Overstory Monthly LAI    8 = 12 12 12 12 12 12 12 12 12 12 12 12
Understory Monthly LAI   8 = 3.0 3.0 3.0 3.0 3.0 3.0 3.0 3.0 3.0 3.0 3.0 3.0
Maximum Resistance       8 = 2000 2000  
Minimum Resistance       8 = 1333.2 855.54   
Moisture Threshold       8 = 0.33 0.13     
Vapor Pressure Deficit   8 = 4000 4000     
Rpc                      8 = .108 .108
Overstory Monthly Alb    8 = 0.14 0.14 0.14 0.13 0.13 0.12 0.11 0.11 0.12 0.13 0.14 0.14
Understory Monthly Alb   8 = 0.19 0.19 0.19 0.19 0.19 0.19 0.19 0.19 0.19 0.19 0.19 0.19
Number of Root Zones     8 = 3 		   
Root Zone Depths         8 = 0.10 0.25 0.40    
Overstory Root Fraction  8 = 0.20 0.40 0.40      
Understory Root Fraction 8 = 0.40 0.60 0.00        

Vegetation Description   9 = Regrowth Vegetation
Impervious Fraction      9 = 0.0
Detention Fraction       9 = 0
Detention Decay          9 = 0
Overstory Present        9 = FALSE        
Understory Present       9 = TRUE             
Fractional Coverage      9 =          
Hemi Fract Coverage      9 =
Clumping Factor          9 =
Leaf Angle A             9 =
Leaf Angle B             9 =
Scattering Parameter     9 =
Trunk Space              9 =            
Aerodynamic Attenuation  9 =           
Radiation Attenuation    9 =          
Max Snow Int Capacity    9 =		  
Snow Interception Eff    9 =               
Mass Release Drip Ratio  9 =              
Height                   9 =  1.0    
Overstory Monthly LAI    9 = 
Understory Monthly LAI   9 = 0.5 0.5 0.5 0.5 0.5 0.5 0.5 0.5 0.5 0.5 0.5 0.5
Maximum Resistance       9 =  600  
Minimum Resistance       9 =  220   
Moisture Threshold       9 =  0.33     
Vapor Pressure Deficit   9 =  4000     
Rpc                      9 =  .108
Overstory Monthly Alb    9 = 
Understory Monthly Alb   9 = 0.2 0.2 0.2 0.19 0.18 0.17 0.16 0.16 0.17 0.18 0.19 0.2
Number of Root Zones     9 = 3 		   
Root Zone Depths         9 =  0.10 0.25 0.40   
Overstory Root Fraction  9 =  0.20 0.40 0.40     
Understory Root Fraction 9 =  0.40 0.60 0.00     

Vegetation Description   10 = Clear-cuts  
Impervious Fraction      10 = 0.0
Detention Fraction       10 = 0
Detention Decay          10 = 0
Overstory Present        10 = FALSE        
Understory Present       10 = TRUE             
Fractional Coverage      10 =          
Hemi Fract Coverage      10 =
Clumping Factor          10 =
Leaf Angle A             10 =
Leaf Angle B             10 =
Scattering Parameter     10 =
Trunk Space              10 =            
Aerodynamic Attenuation  10 =           
Radiation Attenuation    10 =          
Max Snow Int Capacity    10 =		  
Snow Interception Eff    10 =               
Mass Release Drip Ratio  10 =              
Height                   10 = 0.5   
Overstory Monthly LAI    10 = 
Understory Monthly LAI   10 = 0.5 0.5 0.5 0.5 0.5 6.0 6.0 6.0 6.0 0.5 0.5 0.5
Maximum Resistance       10 = 600  
Minimum Resistance       10 = 280    
Moisture Threshold       10 = 0.33      
Vapor Pressure Deficit   10 = 4000      
Rpc                      10 = .108
Overstory Monthly Alb    10 = 
Understory Monthly Alb   10 = 0.19 0.19 0.19 0.19 0.19 0.19 0.19 0.19 0.19 0.19 0.19 0.19
Number of Root Zones     10 = 3 		   
Root Zone Depths         10 = 0.10 0.25 0.40    
Overstory Root Fraction  10 = 0.20 0.40 0.40      
Understory Root Fraction 10 = 0.40 0.60 0.00    

Vegetation Description   11 = Rock
Impervious Fraction      11 = 0.0
Detention Fraction       11 = 0
Detention Decay          11 = 0
Overstory Present        11 = FALSE        
Understory Present       11 = FALSE            
Fractional Coverage      11 =        
Hemi Fract Coverage      11 =
Clumping Factor          11 =
Leaf Angle A             11 =
Leaf Angle B             11 =
Scattering Parameter     11 =
Trunk Space              11 =             
Aerodynamic Attenuation  11 =         
Radiation Attenuation    11 = 
Max Snow Int Capacity    11 = 
Snow Interception Eff    11 = 
Mass Release Drip Ratio  11 = 
Height                   11 =   
Overstory Monthly LAI    11 = 
Understory Monthly LAI   11 = 
Maximum Resistance       11 =  
Minimum Resistance       11 = 
Moisture Threshold       11 =  
Vapor Pressure Deficit   11 =  
Rpc                      11 = 
Overstory Monthly Alb    11 = 
Understory Monthly Alb   11 = 
Number of Root Zones     11 = 3 		   
Root Zone Depths         11 = 0.10 0.25 0.40  
Overstory Root Fraction  11 = 0.20 0.40 0.40
Understory Root Fraction 11 = 0.40 0.60 0.00      

Vegetation Description   12 = Wetlands
Impervious Fraction      12 = 0.0
Detention Fraction       12 = 0
Detention Decay          12 = 0
Overstory Present        12 = FALSE        
Understory Present       12 = TRUE           
Fractional Coverage      12 = 
Hemi Fract Coverage      12 =
Clumping Factor          12 =
Leaf Angle A             12 =
Leaf Angle B             12 =
Scattering Parameter     12 =
Trunk Space              12 = 
Aerodynamic Attenuation  12 = 
Radiation Attenuation    12 = 
Max Snow Int Capacity    12 = 
Snow Interception Eff    12 = 
Mass Release Drip Ratio  12 = 
Height                   12 = 0.5
Overstory Monthly LAI    12 = 
Understory Monthly LAI   12 = 0.5 0.5 0.5 0.5 0.5 6.0 6.0 6.0 6.0 0.5 0.5 0.5 
Maximum Resistance       12 = 600
Minimum Resistance       12 = 200
Moisture Threshold       12 = 0.33
Vapor Pressure Deficit   12 = 4000
Rpc                      12 = 0.108
Overstory Monthly Alb    12 = 
Understory Monthly Alb   12 = 0.19 0.19 0.19 0.17 0.17 0.16 0.16 0.16 0.16 0.17 0.19 0.19
Number of Root Zones     12 = 3		   
Root Zone Depths         12 = 0.10 0.25 0.40  
Overstory Root Fraction  12 = 0.20 0.40 0.40
Understory Root Fraction 12 = 0.4 0.6 0.0  

Vegetation Description   13 = Shoreline
Impervious Fraction      13 = 0.0
Detention Fraction       13 = 0
Detention Decay          13 = 0
Overstory Present        13 = FALSE        
Understory Present       13 = TRUE             
Fractional Coverage      13 = 
Hemi Fract Coverage      13 =
Clumping Factor          13 =
Leaf Angle A             13 =
Leaf Angle B             13 =
Scattering Parameter     13 =
Trunk Space              13 = 
Aerodynamic Attenuation  13 = 
Radiation Attenuation    13 = 
Max Snow Int Capacity    13 = 
Snow Interception Eff    13 = 
Mass Release Drip Ratio  13 = 
Height                   13 = 0.5
Overstory Monthly LAI    13 = 
Understory Monthly LAI   13 = 0.5 0.5 0.5 0.5 0.5 6.0 6.0 6.0 6.0 0.5 0.5 0.5 
Maximum Resistance       13 = 600 
Minimum Resistance       13 = 200 
Moisture Threshold       13 = 0.33       
Vapor Pressure Deficit   13 = 4000      
Rpc                      13 = .108
Overstory Monthly Alb    13 = 
Understory Monthly Alb   13 = 0.19 0.19 0.19 0.17 0.17 0.16 0.16 0.16 0.16 0.17 0.19 0.19
Number of Root Zones     13 = 3 		   
Root Zone Depths         13 = 0.10 0.25 0.40    
Overstory Root Fraction  13 = 0.20 0.40 0.40
Understory Root Fraction 13 = 0.40 0.60 0.00       

Vegetation Description   14 = Water 
Impervious Fraction      14 = 0.0
Detention Fraction       14 = 0
Detention Decay          14 = 0
Overstory Present        14 = FALSE        
Understory Present       14 = FALSE            
Fractional Coverage      14 = 
Hemi Fract Coverage      14 =
Clumping Factor          14 =
Leaf Angle A             14 =
Leaf Angle B             14 =
Scattering Parameter     14 =
Trunk Space              14 = 
Aerodynamic Attenuation  14 = 
Radiation Attenuation    14 = 
Max Snow Int Capacity    14 = 
Snow Interception Eff    14 = 
Mass Release Drip Ratio  14 = 
Height                   14 = 
Overstory Monthly LAI    14 = 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0
Understory Monthly LAI   14 = 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0
Maximum Resistance       14 = 
Minimum Resistance       14 = 
Moisture Threshold       14 = 
Vapor Pressure Deficit   14 = 
Rpc                      14 = 
Overstory Monthly Alb    14 = 0.00 0.00 0.00 0.00 0.00 0.00 0.00 0.00 0.00 0.00 0.00 0.00
Understory Monthly Alb   14 = 0.00 0.00 0.00 0.00 0.00 0.00 0.00 0.00 0.00 0.00 0.00 0.00
Number of Root Zones     14 = 3 		   
Root Zone Depths         14 = 0.10 0.25 0.40  
Overstory Root Fraction  14 = 0.20 0.40 0.40
Understory Root Fraction 14 = 0.00 0.00 0.00      

################################################################################
# MODEL OUTPUT SECTION
################################################################################
[OUTPUT]                                  # Information what to output when
Output Directory           = /nfs/electric/raid/ning/trash/tutorial3.1/output/
Initial State Directory    = /nfs/electric/raid/ning/Test_SpringBrook/modelstate/

################ PIXEL DUMPS ###################################################

Number of Output Pixels    = 0

# For each pixel make a key-entry pair as indicated below, varying the 
# number for the output pixel  (1, .. , Number of Output Pixel)

North Coordinate         1 = 
East Coordinate          1 = 
Name                     1 = 

################ MODEL STATE ###################################################                
Number of Model States     =  4            # Number of model states to dump

# For each model state make a key-entry pair as indicated below, varying the 
# number for the model state dump (1, .. , Number of Model States)

State Date               1 = 01/01/1998-00  # Time for model state dump
State Date               2 = 01/01/1999-00  # Time for model state dump
State Date               3 = 01/01/2000-00  # Time for model state dump
State Date               4 = 01/01/2001-00  # Time for model state dump
################ MODEL MAPS ####################################################

Number of Map Variables    = 3             # Number of different variables for
                                          # which you want to output maps

# For each of the variables make a block like the one that follows, varying
# the number of the variable (n = 1, .. , Number of Map Variables)

Map Variable             1 = 201          # ID of the variable to output
Number of Maps           1 = 12           
Map Date 1               1 = 12/13/1995-03
Map Date 2               1 = 12/13/1995-06 
Map Date 3               1 = 12/13/1995-09 
Map Date 4               1 = 12/13/1995-12 
Map Date 5               1 = 12/13/1995-15 
Map Date 6               1 = 12/13/1995-18 
Map Date 7               1 = 12/13/1995-21 
Map Date 8               1 = 12/14/1995-00 
Map Date 9               1 = 12/14/1995-03 
Map Date 10              1 = 12/14/1995-06 
Map Date 11              1 = 12/14/1995-09 
Map Date 12              1 = 12/14/1995-12 

Map Variable             2 = 401          # ID of the variable to output
Number of Maps           2 = 12           
Map Date 1               2 = 8/13/1999-03
Map Date 2               2 = 8/13/1999-06 
Map Date 3               2 = 8/13/1999-09 
Map Date 4               2 = 8/13/1999-12 
Map Date 5               2 = 8/13/1999-15 
Map Date 6               2 = 8/13/1999-18 
Map Date 7               2 = 8/13/1999-21 
Map Date 8               2 = 8/14/1999-00 
Map Date 9               2 = 8/14/1999-03 
Map Date 10              2 = 8/14/1999-06 
Map Date 11              2 = 8/14/1999-09 
Map Date 12              2 = 8/14/1999-12 

Map Variable             3 = 501          # ID of the variable to output
Map Layer                3 = 1
Number of Maps           3 = 12       
Map Date 1               3 = 12/13/1999-03
Map Date 2               3 = 12/13/1999-06 
Map Date 3               3 = 12/13/1999-09 
Map Date 4               3 = 12/13/1999-12 
Map Date 5               3 = 12/13/1999-15 
Map Date 6               3 = 12/13/1999-18 
Map Date 7               3 = 12/13/1999-21 
Map Date 8               3 = 12/14/1999-00 
Map Date 9               3 = 12/14/1999-03 
Map Date 10              3 = 12/14/1999-06 
Map Date 11              3 = 12/14/1999-09 
Map Date 12              3 = 12/14/1999-12 

################ MODEL IMAGES ##################################################

Number of Image Variables  = 0            # Number of variables for which you 
                                          # would like to output images

# For each of the variables make a block like the one that follows, varying
# the number of the variable (n = 1, .. , Number of Image Variables)

Image Variable        1 = 501                # ID of the variable to output
Image Layer           1 = 1                # If the variable exists for a number
					  # of layers, specify the layers here
					  # with the top layer = 1
Image Start           1 =                 # First timestep for which to output
                                          # an image
Image End             1 =                 # Last timestep for which to output
                                          # an image
Image Interval        1 =                 # Time interval between images (hours)
Image Upper Limit     1 =                 # All values in the output equal to or
                                          # greater than this limit will be set 
                                          # to 255
Image Lower Limit     1 =                 # All values in the output equal to or
                                          # smaller than this limit will be set 
                                          # to 0
################ GRAPHIC IMAGES ##################################################

Number of Graphics      =  0               # Number of variables for which you 
                                          # would like to output images
Graphics ID           1 = 19                # ID of the variable to output
Graphics ID           1 = 22
Graphics ID           2 = 23
Graphics ID           3 = 24
Graphics ID           4 = 25
Graphics ID           5 = 43
Graphics ID           6 = 44
Graphics ID           7 = 8
Graphics ID           8 = 2
Graphics ID           9 = 50
Graphics ID          10 = 1

# 1	SWE (mm)
# 2	Water Table Depth (mm)
# 3	Digital Elevation Model (m)
# 4	Vegetation Class (index #)
# 5	Soil Class (index #)
# 6	Soil Depth (mm)
# 7	Precipitation at current time step (mm/time step)
# 8	Incoming Shortwave (Beam and Diffuse) (W/sqm)
# 9	Intercepted Snow (mm)
# 10	Snow Surface Temp (C)
# 11	Cold Content of snow entire snow pack (kJ)
# 12	Snow Melt (as Outflow minus Precip, can be negative) (mm/time step)
# 13	Snow Pack Outflow (mm/time step)
# 14	Saturated Subsurface Flow (mm/time step)
# 15	Overland Flow(mm)
# 16	Total Evapotranspiration (soil + all veg layers)
# 17	Ground Snow pack vapor flux (mm)
# 18	Intercepted snow pack vapor flux (mm)
# 19    Soil Moisture (Surface Layer) % of saturation (i.e. porosity)
# 20    Soil Moisture (2nd Layer) % of saturation (i.e. porosity)
# 21    Soil Moisture (3rd Layer) % of saturation (i.e. porosity)
# 22    Accumulated Precip (mm)
# 23    air temperature (C)
# 24    wind speed (m/s)
# 25    relative humidity
# 26    Prism Precip Field (mm)
# 31    Overstory Transpiration (mm)
# 32    Understory Transpirtation (mm)
# 33    Soil Evaporation (mm)
# 34    Overstory Evaporation (mm)
# 35    Understory Evaportation (mm)
# 41    Sky View Factor (%)
# 42    Shade Map (%)
# 43    Direct Beam Shortwave Rad (W/sqm)
# 44    Diffuse Beam Shortwave Rad (W/sqm)
# 45    Aspect (degrees)
# 46    Slope (percent)
# 50    Channel Subsurface Interception (mm)
# 51    Road Subsurface Interception (mm)
# WARNING Use soil mositure layers with caution, to minimize calculations during redraw
# DHSVM does not check to make sure that the assigned soil layer exists

################################################################################
# END OF INPUT FILE
################################################################################
[End]                                     # This is probably not needed, but 
                                          # just in case (to close the previous
                                          # section)

</pre></body></html>